From 6e7e1b7172813fc4ecb60597f903dd21a4616159 Mon Sep 17 00:00:00 2001
From: John Ogness <john.ogness@linutronix.de>
Date: Tue, 19 Dec 2017 11:16:28 +0100
Subject: update yocto-advanced: sync to devel/manut/yocto

The devel/manut/yocto heavily diverted from master. Sync
with latest version 8cd4956a9b48a316eab6dc6d1b1f6cd51362fecf.

Signed-off-by: John Ogness <john.ogness@linutronix.de>
---
 .../yocto-advanced/yocto-u-boot-integration.tex    | 27 +---------------------
 1 file changed, 1 insertion(+), 26 deletions(-)

(limited to 'distribution/yocto-advanced/yocto-u-boot-integration.tex')

diff --git a/distribution/yocto-advanced/yocto-u-boot-integration.tex b/distribution/yocto-advanced/yocto-u-boot-integration.tex
index 6b1421e..5617839 100644
--- a/distribution/yocto-advanced/yocto-u-boot-integration.tex
+++ b/distribution/yocto-advanced/yocto-u-boot-integration.tex
@@ -5,31 +5,6 @@ add
 PREFERRED_PROVIDER_virtual/bootloader = "u-boot"
 PREFERRED_PROVIDER_virtual/u-boot = "u-boot"
 \end{verbatim}
-to meta-mini/machine/beaglebone-black.conf
+to meta-mybsp/machine/beaglebone-black.conf
 \end{frame}
 
-\subsection{generate a sdcard image}
-\begin{frame}[fragile]
-\frametitle{sdcard generation}
-create the file: 'meta-mini/classes/image\_sdcard.bbclass':
-\begin{verbatim}
-inherit image_types
-
-IMAGE_BOOTLOADER ?= "u-boot"
-
-# Handle u-boot suffixes
-UBOOT_SUFFIX ?= "bin"
-UBOOT_PADDING ?= "0"
-UBOOT_SUFFIX_SDCARD ?= "${UBOOT_SUFFIX}"
-
-# Linux bootstream
-IMAGE_DEPENDS_linux.sb = "virtual/kernel:do_deploy"
-
-# Boot partition volume id
-BOOTDD_VOLUME_ID ?= "Boot ${MACHINE}"
-# Boot partition size [in KiB]
-BOOT_SPACE ?= "8192"
-# Set alignment to 4MB [in KiB]
-IMAGE_ROOTFS_ALIGNMENT = "4096"
-\end{verbatim}
-\end{frame}
-- 
cgit v1.2.3

