From 4a056623cda47030eba61cfb1e426148af8eb59a Mon Sep 17 00:00:00 2001
From: John Ogness <john.ogness@linutronix.de>
Date: Mon, 13 Nov 2017 13:21:14 +0100
Subject: yocto-basic: update

+ update yocto version in some slides
+ add missing slides
+ fix typos

Signed-off-by: Volker Haspel <volker.haspel@linutronix.de>
Signed-off-by: John Ogness <john.ogness@linutronix.de>
---
 distribution/yocto-basic/yocto-adt.tex | 109 ++++++++++++++++-----------------
 1 file changed, 52 insertions(+), 57 deletions(-)

(limited to 'distribution/yocto-basic/yocto-adt.tex')

diff --git a/distribution/yocto-basic/yocto-adt.tex b/distribution/yocto-basic/yocto-adt.tex
index 17d0733..250f6a9 100644
--- a/distribution/yocto-basic/yocto-adt.tex
+++ b/distribution/yocto-basic/yocto-adt.tex
@@ -1,6 +1,6 @@
 \subsection{ADT}
 \begin{frame}
-\frametitle{Yocto ADT (Application Development Kit}
+\frametitle{Yocto ADT (Application Development Kit)}
 Core Components
 \vspace{2em}
 \begin{itemize}
@@ -45,13 +45,11 @@ poky/build % bitbake meta-toolchain
 poky/build % bitbake -c populate_sdk core-image-minimal
 \end{verbatim}
 \vspace{2em}
-\pause
 to install the toolchain:
 \begin{verbatim}
 % ./tmp/deploy/sdk/poky-glibc-x86\_64-meta-toolchain-i586-toolchain-2.0.sh
 Enter target directory for SDK (default: /opt/poky/2.0): /home/devel/sdk
 \end{verbatim}
-\pause
 to use the toolchain:
 \begin{verbatim}
 source /home/devel/sdk/environment-setup-i586-poky-linux
@@ -75,58 +73,57 @@ poky/build % bitbake meta-ide-support
 \vspace{2em}
 \end{frame}
 
-\begin{frame}[fragile]
-\frametitle{build ADT installer script}
-\begin{verbatim}
-poky/build % bitbake adt-installer
-poky/build % cp tmp/deploy/sdk/adt_installer.tar.bz2 ~/
-poky/build % cd
-% cp tmp/deploy/sdk/adt_installer.tar.bz2 ~/
-% tar xjf adt_installer.tar.bz2
-% cd adt-installer
-\end{verbatim}
-\end{frame}
-
-\begin{frame}
-\frametitle{configure ADT installer}
-general configuration
-\begin{description}
-\item[YOCTOADT\_REPO] http repo with rootfs images and ipkg packages.
-	Needs to match the layout from 'http://adtrepo.yoctoproject.org'
-\item[YOCTOADT\_TARGETS] machine target architectures to setup cross SDKs
-\item[YOCTOADT\_QEMU] install qemu? \[Y/N\]
-\item[YOCTOADT\_NFS\_UTIL] needed for eclipse \[Y/N\]
-\end{description}
-\end{frame}
-
-\begin{frame}
-\frametitle{configure ADT installer \#2}
-configuration for each supported BSP
-\begin{description}
-\item[YOCTOADT\_TARGET\_MACHINE\_<arch>] qemu that should be used, e.g. qemux86
-\item[YOCTOADT\_ROOTFS\_<arch>] rfs images that should be used, e.g. sato-sdk
-\item[YOCTOADT\_TARGET\_SYSROOT\_<arch>] needs to match above variable
-\item[YOCTOADT\_TARGET\_SYSROOT\_LOC\_<arch>] path where the sysroot will be
-	stored
-\end{description}
-\end{frame}
-
-\begin{frame}[fragile]
-\frametitle{run ADT installer}
-\begin{verbatim}
-adt-installer % ./adt_installer
-Please enter the install location (default: /opt/poky/2.0): <return>
-...
-[ADT_INST] Please enter your selections here:
-S<return>
-...
-\end{verbatim}
-\pause
-to use the ADT, the environment needs to be sourced:
-\begin{verbatim}
-% .  /opt/poky/2.0/environment-setup-i586-poky-linux
-\end{verbatim}
-\end{frame}
+%\begin{frame}[fragile]
+%\frametitle{build ADT installer script}
+%\begin{verbatim}
+%poky/build % bitbake adt-installer
+%poky/build % cp tmp/deploy/sdk/adt_installer.tar.bz2 ~/
+%poky/build % cd
+%% cp tmp/deploy/sdk/adt_installer.tar.bz2 ~/
+%% tar xjf adt_installer.tar.bz2
+%% cd adt-installer
+%\end{verbatim}
+%\end{frame}
+%
+%\begin{frame}
+%\frametitle{configure ADT installer}
+%general configuration
+%\begin{description}
+%\item[YOCTOADT\_REPO] http repo with rootfs images and ipkg packages.
+%	Needs to match the layout from 'http://adtrepo.yoctoproject.org'
+%\item[YOCTOADT\_TARGETS] machine target architectures to setup cross SDKs
+%\item[YOCTOADT\_QEMU] install qemu? \[Y/N\]
+%\item[YOCTOADT\_NFS\_UTIL] needed for eclipse \[Y/N\]
+%\end{description}
+%\end{frame}
+%
+%\begin{frame}
+%\frametitle{configure ADT installer \#2}
+%configuration for each supported BSP
+%\begin{description}
+%\item[YOCTOADT\_TARGET\_MACHINE\_<arch>] qemu that should be used, e.g. qemux86
+%\item[YOCTOADT\_ROOTFS\_<arch>] rfs images that should be used, e.g. sato-sdk
+%\item[YOCTOADT\_TARGET\_SYSROOT\_<arch>] needs to match above variable
+%\item[YOCTOADT\_TARGET\_SYSROOT\_LOC\_<arch>] path where the sysroot will be
+%	stored
+%\end{description}
+%\end{frame}
+%
+%\begin{frame}[fragile]
+%\frametitle{run ADT installer}
+%\begin{verbatim}
+%adt-installer % ./adt_installer
+%Please enter the install location (default: /opt/poky/2.0): <return>
+%...
+%[ADT_INST] Please enter your selections here:
+%S<return>
+%...
+%\end{verbatim}
+%to use the ADT, the environment needs to be sourced:
+%\begin{verbatim}
+%% .  /opt/poky/2.0/environment-setup-i586-poky-linux
+%\end{verbatim}
+%\end{frame}
 
 \begin{frame}[fragile]
 \frametitle{ADT \& Eclipse}
@@ -136,7 +133,6 @@ install and start eclipse:
 % tar xzf eclipse-*.tar.gz
 % ./eclipse/eclipse
 \end{verbatim}
-\pause
 add the yocto update-site (Help, Install New Software, Add\dots)
 \begin{verbatim}
 http://downloads.yoctoproject.org/releases/eclipse-plugin/1.9/kepler/
@@ -145,7 +141,6 @@ select and install all components, by clicking
 
 'Next, Next, Accept Licenses, Finish, Accept installing from insecure source,
 and accept to restart eclipse'
-\pause
 goto 'Help, Install New Software, Add\dots' again and
 select 'Kepler' as update site and select 'Linux Tools' and
 'Mobile and Device Development'; select 'Next' until you can
-- 
cgit v1.2.3

