From ea793b23c98403cefb38670d02a778b843bdf997 Mon Sep 17 00:00:00 2001
From: John Ogness <john.ogness@linutronix.de>
Date: Thu, 19 Apr 2018 11:03:45 +0200
Subject: replace *all* tabs with spaces

There are times when tabs are allowed and times when they are not.
Let's just simply never use tabs for anything. This makes it easy
to find presentations where tabs were accidentally inserted.

Signed-off-by: John Ogness <john.ogness@linutronix.de>
---
 distribution/yocto-basic/yocto-workflow.tex | 214 ++++++++++++++--------------
 1 file changed, 107 insertions(+), 107 deletions(-)

(limited to 'distribution/yocto-basic/yocto-workflow.tex')

diff --git a/distribution/yocto-basic/yocto-workflow.tex b/distribution/yocto-basic/yocto-workflow.tex
index 3d9651a..efa3a52 100644
--- a/distribution/yocto-basic/yocto-workflow.tex
+++ b/distribution/yocto-basic/yocto-workflow.tex
@@ -74,8 +74,8 @@ layers should be grouped by functionality
 \end{frame}
 
 \begin{frame}[fragile]
-	\frametitle{directory layout}
-	\begin{verbatim}
+\frametitle{directory layout}
+\begin{verbatim}
 poky
 ├── bitbake
 ├── documentation
@@ -107,8 +107,8 @@ poky
 VAR = "value"
 \end{verbatim}
 \begin{itemize}
-	\item normal assignment
-	\item values need to be surrounded by double quotes
+\item normal assignment
+\item values need to be surrounded by double quotes
 \end{itemize}
 \end{frame}
 
@@ -119,8 +119,8 @@ VAR ?= "1"
 VAR ?= "2"
 \end{verbatim}
 \begin{itemize}
-	\item VAR is set to "1" in this example
-	\item if there are multiple assignments using ?= the first one is used
+\item VAR is set to "1" in this example
+\item if there are multiple assignments using ?= the first one is used
 \end{itemize}
 \end{frame}
 
@@ -131,8 +131,8 @@ VAR ??= "1"
 VAR ??= "2"
 \end{verbatim}
 \begin{itemize}
-	\item VAR is set to "2" in this example
-	\item if there are multiple assignments using ??= the last one is used
+\item VAR is set to "2" in this example
+\item if there are multiple assignments using ??= the last one is used
 \end{itemize}
 \end{frame}
 
@@ -146,8 +146,8 @@ VAR_B ?= "12"
 VAR_B ??= "34"
 \end{verbatim}
 \begin{itemize}
-	\item VAR\_A contains "34"
-	\item VAR\_B contains "12"
+\item VAR\_A contains "34"
+\item VAR\_B contains "12"
 \end{itemize}
 \end{frame}
 
@@ -161,7 +161,7 @@ VAR ?= "78"
 VAR ??= "78"
 \end{verbatim}
 \begin{itemize}
-	\item VAR contains "56"
+\item VAR contains "56"
 \end{itemize}
 \end{frame}
 
@@ -176,9 +176,9 @@ VAR_A = "33"
 echo ${VAR_A} ${VAR_B} ${VAR_C}
 \end{verbatim}
 \begin{itemize}
-	\item 33 B:33 C:22
-	\item the content of VAR\_C is expanded immediately on assignment
-	\item the content of VAR\_B is expanded on use
+\item 33 B:33 C:22
+\item the content of VAR\_C is expanded immediately on assignment
+\item the content of VAR\_B is expanded on use
 \end{itemize}
 \end{frame}
 
@@ -191,9 +191,9 @@ VAR_B = "56"
 VAR_B =+ "78"
 \end{verbatim}
 \begin{itemize}
-	\item VAR\_A contains "12 34"
-	\item VAR\_B contains "78 56"
-	\item there are spaces between the appended values
+\item VAR\_A contains "12 34"
+\item VAR\_B contains "78 56"
+\item there are spaces between the appended values
 \end{itemize}
 \end{frame}
 
@@ -206,9 +206,9 @@ VAR_B = "56"
 VAR_B =. "78"
 \end{verbatim}
 \begin{itemize}
-	\item VAR\_A contains "1234"
-	\item VAR\_B contains "7856"
-	\item there are no spaces between the appended values
+\item VAR\_A contains "1234"
+\item VAR\_B contains "7856"
+\item there are no spaces between the appended values
 \end{itemize}
 \end{frame}
 
@@ -232,8 +232,8 @@ VAR_append = "56"
 VAR_prepend = "12"
 \end{verbatim}
 \begin{itemize}
-	\item VAR contains "123456"
-	\item there are no spaces between the appended values
+\item VAR contains "123456"
+\item there are no spaces between the appended values
 \end{itemize}
 \end{frame}
 
@@ -245,7 +245,7 @@ VAR = "foo"
 VAR_string1 = "bar"
 \end{verbatim}
 \begin{itemize}
-	\item if string1 is listed in OVERRIDES, use "bar" for value of VAR, otherwise use "foo"
+\item if string1 is listed in OVERRIDES, use "bar" for value of VAR, otherwise use "foo"
 \end{itemize}
 \end{frame}
 
@@ -255,7 +255,7 @@ VAR_string1 = "bar"
 VAR[some_flag]="foo"
 \end{verbatim}
 \begin{itemize}
-	\item associate a subsidiary flag value to a variable
+\item associate a subsidiary flag value to a variable
 \end{itemize}
 \end{frame}
 
@@ -268,8 +268,8 @@ B = "2"
 A2 = "Y"
 \end{verbatim}
 \begin{itemize}
-	\item Key expansion happens just before BitBake expands overrides.
-	\item A2 contains "X"
+\item Key expansion happens just before BitBake expands overrides.
+\item A2 contains "X"
 \end{itemize}
 \end{frame}
 
@@ -413,8 +413,8 @@ $ bitbake -e <recipe-name> | grep FILESPATH
 \begin{frame}
 \frametitle{SRC\_URI patch options}
 \begin{itemize}
-	\item patches are applied in the order they appear in SRC\_URI
-	\item quilt is used to apply the patches
+\item patches are applied in the order they appear in SRC\_URI
+\item quilt is used to apply the patches
 \end{itemize}
 \begin{description}
 \item[apply=no] apply patch or not; default is yes
@@ -497,10 +497,10 @@ Same as include, but returns an error, if include file not found.
 \begin{frame}
 \frametitle{basics}
 \begin{itemize}
-	\item are typically used to modify or extend the functionality of the base
-		recipe
-	\item it's recommended by the Yocto project to use bbappend files instead
-		of copying and modyfiing a recipe in an own layer
+\item are typically used to modify or extend the functionality of the base
+        recipe
+\item it's recommended by the Yocto project to use bbappend files instead
+        of copying and modyfiing a recipe in an own layer
 \end{itemize}
 \end{frame}
 
@@ -516,8 +516,8 @@ an append file must be named after the base package:
 \begin{frame}
 \frametitle{basics}
 \begin{itemize}
-	\item python can be used to write functions
-	\item e.g. write your own image generation class
+\item python can be used to write functions
+\item e.g. write your own image generation class
 \end{itemize}
 \end{frame}
 
@@ -525,17 +525,17 @@ an append file must be named after the base package:
 \begin{frame}
 \frametitle{basics}
 \begin{itemize}
-	\item are defined and ordered in classes
-	\item can be overridden by classes and recipes
+\item are defined and ordered in classes
+\item can be overridden by classes and recipes
 \end{itemize}
 \end{frame}
 
 \begin{frame}
-	\frametitle{download \& patch}
+\frametitle{download \& patch}
 \begin{description}
 \item [do\_checkuri] validates the SRC\_URI value
 \item [do\_checkuriall] validates the SRC\_URI value for all recipes required
-	to build a target"
+        to build a target"
 \item [do\_fetch] fetches the source code
 \item [do\_fetchall] fetches all remote sources required to build a target
 \item [do\_unpack] unpacks the source code into a working directory
@@ -544,18 +544,18 @@ an append file must be named after the base package:
 \end{frame}
 
 \begin{frame}
-	\frametitle{configure \& compile}
+\frametitle{configure \& compile}
 \begin{description}
 \item [do\_configure] configures the source by enabling and disabling any
-	build-time and configuration options for the software being built
+        build-time and configuration options for the software being built
 \item [do\_configure\_ptest\_base] configures the runtime test suite included
-	in the software being built
+        in the software being built
 \item [do\_compile] compiles the source in the compilation directory
 \item [do\_install] copies files from the compilation directory to a holding
-	area
+        area
 \item [do\_populate\_sysroot] copies a subset of files installed by
-	do\_install into the sysroot in order to make them available to other
-	recipes
+        do\_install into the sysroot in order to make them available to other
+        recipes
 \end{description}
 \end{frame}
 
@@ -563,34 +563,34 @@ an append file must be named after the base package:
 \frametitle{packaging}
 \begin{description}
 \item [do\_packagedata] creates package metadata used by the build system to
-	generate the final packages
+        generate the final packages
 \item [do\_package] analyzes the content of the holding area and splits it
-	into subsets based on available packages and files
+        into subsets based on available packages and files
 \item [do\_package\_write] creates the actual packages and places them in the
-	Package Feed area
+        Package Feed area
 \item [do\_package\_write\_deb] creates the actual DEB packages and places
-	them in the Package Feed area
+        them in the Package Feed area
 \item [do\_package\_write\_ipk] creates the actual IPK packages and places
-	them in the Package Feed area
+        them in the Package Feed area
 \item [do\_package\_write\_rpm] creates the actual RPM packages and places
-	them in the Package Feed area
+        them in the Package Feed area
 \item [do\_package\_write\_tar] creates tar archives for packages and places
-	them in the Package Feed area
+        them in the Package Feed area
 \item [do\_package\_index] creates or updates the index in the Package Feed
-	area
+        area
 \end{description}
 \end{frame}
 
 \begin{frame}
-	\frametitle{deploy}
+\frametitle{deploy}
 \begin{description}
 \item [do\_rootfs] creates the root filesystem (file and directory structure)
-	for an image
+        for an image
 \item [do\_vmdkimg] creates a .vmdk image for use with VMware and compatible
-	virtual machine hosts"
+        virtual machine hosts"
 \item [do\_deploy] writes deployable output files to the deploy directory
 \item [do\_populate\_sdk] creates the file and directory structure for an
-	installable SDK
+        installable SDK
 \end{description}
 \end{frame}
 
@@ -599,13 +599,13 @@ an append file must be named after the base package:
 \begin{description}
 \item [do\_clean] removes all output files for a target
 \item [do\_cleanall] removes all output files, shared state cache, and
-	downloaded source files for a target
+        downloaded source files for a target
 \item [do\_cleansstate] removes all output files and shared state cache for a
-	target
+        target
 \item [do\_rm\_work] removes work files after the build system has finished
-	with them
+        with them
 \item [do\_rm\_work\_all] top-level task for removing work files after the
-	build system has finished with them
+        build system has finished with them
 \end{description}
 \end{frame}
 
@@ -613,20 +613,20 @@ an append file must be named after the base package:
 \frametitle{kernel}
 \begin{description}
 \item [do\_kernel\_checkout] checks out source/meta branches for a linux-yocto
-	style kernel
+        style kernel
 \item [do\_validate\_branches] ensures that the source/meta branches are on
-	the locations specified by their SRCREV values for a linux-yocto style
-	kernel"
+        the locations specified by their SRCREV values for a linux-yocto style
+        kernel"
 \item [do\_kernel\_configme] assembles the kernel configuration for a
-	linux-yocto style kernel
+        linux-yocto style kernel
 \item [do\_menuconfig] runs 'make menuconfig' for the kernel
 \item [do\_diffconfig] compares the old and new config files after running
-	do\_menuconfig for the kernel
+        do\_menuconfig for the kernel
 \item [do\_savedefconfig] creates a minimal Linux kernel configuration file
 \item [do\_kernel\_configcheck] validates the kernel configuration for a
-	linux-yocto style kernel
+        linux-yocto style kernel
 \item [do\_sizecheck] checks the size of the kernel image against
-	KERNEL\_IMAGE\_MAXSIZE (if set)
+        KERNEL\_IMAGE\_MAXSIZE (if set)
 \end{description}
 \end{frame}
 
@@ -634,12 +634,12 @@ an append file must be named after the base package:
 \frametitle{kernel}
 \begin{description}
 \item [do\_compile\_kernelmodules] compiles loadable modules for the Linux
-	kernel
+        kernel
 \item [do\_strip] strips unneeded sections out of the Linux kernel image
 \item [do\_kernel\_link\_vmlinux] creates a symbolic link in arch/\$arch/boot
-	for vmlinux kernel images
+        for vmlinux kernel images
 \item [do\_bundle\_initramfs] combines an initial ramdisk image and kernel
-	together to form a single image
+        together to form a single image
 \end{description}
 \end{frame}
 
@@ -647,9 +647,9 @@ an append file must be named after the base package:
 \frametitle{licenses}
 \begin{description}
 \item [do\_populate\_lic] writes license information for the recipe that is
-	collected later when the image is constructed
+        collected later when the image is constructed
 \item [do\_spdx] a build stage that takes the source code and scans it on a
-	remote FOSSOLOGY server in order to produce an SPDX document
+        remote FOSSOLOGY server in order to produce an SPDX document
 \end{description}
 \end{frame}
 
@@ -657,11 +657,11 @@ an append file must be named after the base package:
 \frametitle{special stuff}
 \begin{description}
 \item [do\_uboot\_mkimage] creates a uImage file from the kernel for the
-	U-Boot bootloader
+        U-Boot bootloader
 \item [do\_generate\_qt\_config\_file] writes a qt.conf file for building a
-	Qt-based application
+        Qt-based application
 \item [do\_devshell] starts a shell with the environment set up for
-	development/debugging
+        development/debugging
 \item [do\_listtasks] lists all defined tasks for a target
 \end{description}
 \end{frame}
@@ -671,49 +671,49 @@ an append file must be named after the base package:
 \frametitle{basics}
 a machine config is used to describe a board
 \begin{itemize}
-	\item machine configs are stored in the layers: conf/machine/*
-	\item settings can be splitted in different include *.inc files
-	\item e.g. one include for CPU that is used by the SoC inc file,
+\item machine configs are stored in the layers: conf/machine/*
+\item settings can be splitted in different include *.inc files
+\item e.g. one include for CPU that is used by the SoC inc file,
 that is used by the Board .conf file
-	\item the include files can be stored in different layers
+\item the include files can be stored in different layers
 \end{itemize}
 \end{frame}
 
 \begin{frame}
-	\frametitle{u-boot \& kernel}
+\frametitle{u-boot \& kernel}
 \begin{description}
-	\item [UBOOT\_MACHINE] value passed on the make command line when building a
-		U-Boot image
-	\item [UBOOT\_MAKE\_TARGET] target called in the Makefile
-	\item [UBOOT\_ENTRYPOINT] entry point for the U-Boot image
-	\item [PREFERRED\_PROVIDER\_virtual/kernel] default kernel
-	\item [KERNEL\_DEVICETREE] default devicetree
-	\item [KERNEL\_IMAGETYPE] type of kernel to build for a device,
-		defaults to 'zImage'
+\item [UBOOT\_MACHINE] value passed on the make command line when building a
+        U-Boot image
+\item [UBOOT\_MAKE\_TARGET] target called in the Makefile
+\item [UBOOT\_ENTRYPOINT] entry point for the U-Boot image
+\item [PREFERRED\_PROVIDER\_virtual/kernel] default kernel
+\item [KERNEL\_DEVICETREE] default devicetree
+\item [KERNEL\_IMAGETYPE] type of kernel to build for a device,
+        defaults to 'zImage'
 \end{description}
 \end{frame}
 
 \begin{frame}
-	\frametitle{hardware}
+\frametitle{hardware}
 \begin{description}
-	\item[SOC\_FAMILY] groups together machines based upon the same family of SOC
-		(System On Chip)
-	\item [MACHINEOVERRIDES] lists overrides specific to the current machine.
-		By default, this list includes the value of MACHINE. This can be used in
-		recipes; e.g. MACHINEOVERRIDES =. "mymachine" and in the recipe
-		SRC\_URI\_append\_mymachine = "file://mymachine-quirk.patch"
-	\item [MACHINE\_FEATURES] list of hardware features the MACHINE supports
-		\footnote{acpi, alsa, apm, bluetooth, ext2, irda, keyboard, pci, pcmcia,
-		screen, serial, touchscreen, usbgadget, usbhost, wifi}
-	\item [MACHINE\_EXTRA\_RRECOMMENDS] list of machine-specific packages to
-		install as part of the image being built that are not essential for booting
-		the machine. The image being built has no build dependencies on the packages
-		in this list.
+\item[SOC\_FAMILY] groups together machines based upon the same family of SOC
+        (System On Chip)
+\item [MACHINEOVERRIDES] lists overrides specific to the current machine.
+        By default, this list includes the value of MACHINE. This can be used in
+        recipes; e.g. MACHINEOVERRIDES =. "mymachine" and in the recipe
+        SRC\_URI\_append\_mymachine = "file://mymachine-quirk.patch"
+\item [MACHINE\_FEATURES] list of hardware features the MACHINE supports
+\footnote{acpi, alsa, apm, bluetooth, ext2, irda, keyboard, pci, pcmcia,
+        screen, serial, touchscreen, usbgadget, usbhost, wifi}
+\item [MACHINE\_EXTRA\_RRECOMMENDS] list of machine-specific packages to
+        install as part of the image being built that are not essential for booting
+        the machine. The image being built has no build dependencies on the packages
+        in this list.
 \item [SERIAL\_CONSOLE] speed and device for the serial port used to attach
-		the serial console. This variable is given to the kernel as the 'console'
-		parameter. After booting occurs, getty is started on that port so remote
-		login is possible.
-	\end{description}
+        the serial console. This variable is given to the kernel as the 'console'
+        parameter. After booting occurs, getty is started on that port so remote
+        login is possible.
+\end{description}
 \end{frame}
 
 \begin{frame}
@@ -733,6 +733,6 @@ that is used by the Board .conf file
 \item [PREFERRED\_PROVIDER\_virtual/kernel] recommended kernel
 \item [IMAGE\_FSTYPES] formats for the rootfs, e.g. "ext3 tar.bz2"
 \item [IMAGE\_CLASSES] list of classes that all images should inherit, default
-		is image\_types, e.g. to hook in own image generation code
+        is image\_types, e.g. to hook in own image generation code
 \end{description}
 \end{frame}
-- 
cgit v1.2.3

