From 0e7cb133ccdd77a66de18e095815737f5c4e3481 Mon Sep 17 00:00:00 2001
From: John Ogness <john.ogness@linutronix.de>
Date: Tue, 30 Jan 2018 22:46:56 -0600
Subject: module-basics: add device tree to vain

Modern kernels will use device trees for platform devices, so
make vain do the same.

(Also fixup an unnecessary line break.)

Signed-off-by: John Ogness <john.ogness@linutronix.de>
---
 kernel-devel/kernel-debugging/pres_kernel-debugging_en.tex | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

(limited to 'kernel-devel/kernel-debugging/pres_kernel-debugging_en.tex')

diff --git a/kernel-devel/kernel-debugging/pres_kernel-debugging_en.tex b/kernel-devel/kernel-debugging/pres_kernel-debugging_en.tex
index 240eb5a..62624a9 100644
--- a/kernel-devel/kernel-debugging/pres_kernel-debugging_en.tex
+++ b/kernel-devel/kernel-debugging/pres_kernel-debugging_en.tex
@@ -216,8 +216,7 @@ Kernel hacking  --->
 [*]   Early printk
 \end{verbatim}
 \begin{verbatim}
-earlyprintk \
-console=ttyAMA0,115200
+earlyprintk console=ttyAMA0,115200
 \end{verbatim}
 \end{frame}
 
-- 
cgit v1.2.3

