From 4766f6b5e10ed58c210ff9c9d1d048e12d21eebd Mon Sep 17 00:00:00 2001
From: Jan Altenberg <jan@linutronix.de>
Date: Fri, 27 Dec 2013 11:21:25 +0100
Subject: Typo fixes

---
 linux-basics/filesystems/pres_filesystems_en.tex | 17 ++++++++++++++++-
 1 file changed, 16 insertions(+), 1 deletion(-)

(limited to 'linux-basics/filesystems/pres_filesystems_en.tex')

diff --git a/linux-basics/filesystems/pres_filesystems_en.tex b/linux-basics/filesystems/pres_filesystems_en.tex
index 5b1149b..e6339e5 100644
--- a/linux-basics/filesystems/pres_filesystems_en.tex
+++ b/linux-basics/filesystems/pres_filesystems_en.tex
@@ -29,6 +29,10 @@
 \item ReiserFS
 \item XFS
 \end{itemize}
+Filesystem for ''flash based'' block devices:
+\begin{itemize}
+\item F2FS
+\end{itemize}
 \end{frame}
 
 \subsubsection{For flash}
@@ -71,7 +75,8 @@ size of a filesystem
 \begin{itemize}
 \item \textbf{N}o journalling filesystem
 \item A good choice for ''flash-based block devices'', like SD cards or USB
-sticks (ext2 minimizes the number of writes)
+sticks (ext2 minimizes the number of writes), if you have heavy write access. F2FS
+might be an alternative for flash devices
 \item Supported block sizes: 1kb, 2kb, 4kb, 8kb
 \item Max. filesystem size: 32TB (for 8kb blocks)
 \end{itemize}
@@ -112,6 +117,16 @@ sticks (ext2 minimizes the number of writes)
 \end{frame}
 
 \subsubsection{Flash filesystems}
+\begin{frame}
+\frametitle{F2FS}
+\begin{itemize}
+\item F lash F riendly F ilesystem
+\item Available since Linux Kernel 3.8 (backports available back to 3.0)
+\item Not a ''real'' flashfilesystem
+\item For ''NAND flash based'' block devices, like SD, MMC, eMMC, ...
+\end{itemize}
+\end{frame}
+
 \begin{frame}
 \frametitle{JFFS2}
 \begin{itemize}
-- 
cgit v1.2.3

