From 496bcde46e79fa4b61983052e0b08e2db8cba2f3 Mon Sep 17 00:00:00 2001
From: Kurt Kanzenbach <kurt@linutronix.de>
Date: Mon, 18 Feb 2019 11:21:08 +0100
Subject: rt-tests: test your idle system as well

Reason: An Idle system may make use of power management features and introduce
large latencies. This should be also tested.

Signed-off-by: Kurt Kanzenbach <kurt@linutronix.de>
---
 realtime/rt-specialties/pres_rt-specialties_en.tex | 1 +
 1 file changed, 1 insertion(+)

(limited to 'realtime/rt-specialties/pres_rt-specialties_en.tex')

diff --git a/realtime/rt-specialties/pres_rt-specialties_en.tex b/realtime/rt-specialties/pres_rt-specialties_en.tex
index 6fb0fd4..f7fe46b 100644
--- a/realtime/rt-specialties/pres_rt-specialties_en.tex
+++ b/realtime/rt-specialties/pres_rt-specialties_en.tex
@@ -35,6 +35,7 @@ Suitable load scenarios in order to create worst-case situations:
 \item Interrupt Load: flood pinging (''ping -f'')
 \item Serial/Network Load: ''top -d 0'' via console and network shell
 \item Various Load Scenarios: ''stress-ng''
+\item Idle System
 \end{itemize}
 \end{frame}
 
-- 
cgit v1.2.3

