\subsection{ADT}

\begin{frame}
\frametitle{Yocto ADT (Application Development Kit)}
Core Components
\vspace{2em}
\begin{itemize}
\item system root
\item QEMU emulator
\item cross development toolchain
\end{itemize}
\end{frame}

\begin{frame}
\frametitle{Yocto ADT}
Eclipse Plugin
\vspace{2em}
\begin{itemize}
\item roundtrip application development
\item toolchain/system root integration
\item emulated and hardware targets
\item application templates
\item on-target debugging
\end{itemize}
\end{frame}

\begin{frame}
\frametitle{Yocto ADT}
Profiling Tools
\vspace{2em}
\begin{itemize}
\item LatencyTOP
\item PowerTOP
\item OProfile
\item Perf
\item SystemTap
\item Lttng-ust
\end{itemize}
\end{frame}

\begin{frame}[fragile]
\frametitle{Build an External Usable Toolchain}
\begin{verbatim}
bitbake meta-toolchain
\end{verbatim}
or to include headers and static version of all used libraries
\begin{verbatim}
bitbake -c populate_sdk core-image-minimal
\end{verbatim}
To install the toolchain:
\begin{verbatim}
% ./tmp/deploy/sdk/poky-glibc-x86\_64-meta-toolchain-i586-toolchain-2.0.sh
Enter target directory for SDK (default: /opt/poky/2.0): /home/devel/sdk
\end{verbatim}
to use the toolchain:
\begin{verbatim}
source /home/devel/sdk/environment-setup-i586-poky-linux
\end{verbatim}
\end{frame}

\begin{frame}[fragile]
\frametitle{Build an Internal Usable Toolchain}
\begin{verbatim}
bitbake meta-ide-support
\end{verbatim}
\vspace{2em}
\end{frame}

\begin{frame}[fragile]
\frametitle{Export an NFS Root Filesystem}
\begin{verbatim}
runqemu-extract-sdk \
    tmp/deploy/images/qemux86/core-image-minimal-qemux86.tar.bz2 \
    ~/sdk/core-image-minimal
\end{verbatim}
\end{frame}

%\begin{frame}[fragile]
%\frametitle{build ADT installer script}
%\begin{verbatim}
%poky/build % bitbake adt-installer
%poky/build % cp tmp/deploy/sdk/adt_installer.tar.bz2 ~/
%poky/build % cd
%% cp tmp/deploy/sdk/adt_installer.tar.bz2 ~/
%% tar xjf adt_installer.tar.bz2
%% cd adt-installer
%\end{verbatim}
%\end{frame}
%
%\begin{frame}
%\frametitle{configure ADT installer}
%general configuration
%\begin{description}
%\item[YOCTOADT\_REPO] http repo with rootfs images and ipkg packages.
%       Needs to match the layout from 'http://adtrepo.yoctoproject.org'
%\item[YOCTOADT\_TARGETS] machine target architectures to setup cross SDKs
%\item[YOCTOADT\_QEMU] install qemu? \[Y/N\]
%\item[YOCTOADT\_NFS\_UTIL] needed for eclipse \[Y/N\]
%\end{description}
%\end{frame}
%
%\begin{frame}
%\frametitle{configure ADT installer \#2}
%configuration for each supported BSP
%\begin{description}
%\item[YOCTOADT\_TARGET\_MACHINE\_<arch>] qemu that should be used, e.g. qemux86
%\item[YOCTOADT\_ROOTFS\_<arch>] rfs images that should be used, e.g. sato-sdk
%\item[YOCTOADT\_TARGET\_SYSROOT\_<arch>] needs to match above variable
%\item[YOCTOADT\_TARGET\_SYSROOT\_LOC\_<arch>] path where the sysroot will be
%       stored
%\end{description}
%\end{frame}
%
%\begin{frame}[fragile]
%\frametitle{run ADT installer}
%\begin{verbatim}
%adt-installer % ./adt_installer
%Please enter the install location (default: /opt/poky/2.0): <return>
%...
%[ADT_INST] Please enter your selections here:
%S<return>
%...
%\end{verbatim}
%to use the ADT, the environment needs to be sourced:
%\begin{verbatim}
%% .  /opt/poky/2.0/environment-setup-i586-poky-linux
%\end{verbatim}
%\end{frame}

%\begin{frame}[fragile]
%\frametitle{ADT \& Eclipse}
%install and start eclipse:
%\begin{verbatim}
%% wget http://ftp.fau.de/eclipse/technology/epp/downloads/release/kepler/R/eclipse-cpp-kepler-R-linux-gtk.tar.gz
%% tar xzf eclipse-*.tar.gz
%% ./eclipse/eclipse
%\end{verbatim}
%add the yocto update-site (Help, Install New Software, Add\dots)
%\begin{verbatim}
%http://downloads.yoctoproject.org/releases/eclipse-plugin/1.9/kepler/
%\end{verbatim}
%select and install all components, by clicking
%
%'Next, Next, Accept Licenses, Finish, Accept installing from insecure source,
%and accept to restart eclipse'
%goto 'Help, Install New Software, Add\dots' again and
%select 'Kepler' as update site and select 'Linux Tools' and
%'Mobile and Device Development'; select 'Next' until you can
%'Finish' and quit eclipse
%\end{frame}

%\begin{frame}
%\frametitle{configure Eclipse}
%\begin{itemize}
%\item select 'Window, Preferences, Yocto Project ADT'
%\item select 'Standalone pre-built toolchain'
%\item set Toolchain Root Location '/home/devel/sdk'
%\item set Sysroot Location '/home/devel/sdk/core-image-minimal'
%\item use 'native' as 'Target Options'
%\item 'Apply' the Settings and close the dialog with 'OK'
%\end{itemize}
%\end{frame}

%\begin{frame}
%\frametitle{Hello World example}
%\begin{itemize}
%\item select 'File, New, Project\dots'
%\item select 'C/C++, C Project'
%\item select 'Yocto Project ADT Autotools Project, Hello World ANSI C Project'
%\item enter a 'Project name' and select 'Next'
%\item enter 'Basic settings' and select 'Finish'
%\item if opened, close the 'Welcome' window
%\item right click on the root project folder and select 'Reconfigure Project'
%\item right click on the root project folder and select 'Build Project'
%\end{itemize}
%\end{frame}

%\begin{frame}
%\frametitle{remote execution and debugging}
%\begin{itemize}
%\item switch to 'Remote System Explorer' perspective
%\item create a new 'TCF' connection
%\item switch to 'C/C++' perspective and select 'Run / Debug Configurations'
%\item select the preconfigured 'C/C++ Application' and select the correct
%        'Connection'
%\item set 'Remote Absolute File Path' to sth. like '/usr/bin/<yourapp>'
%\item select 'Apply', 'Debug' - Next time you can use this preconfigured debug
%        configuration
%\end{itemize}
%\end{frame}
