From eacbf5bb4d57af21c731f41251015d3b991ad490 Mon Sep 17 00:00:00 2001
From: guest <guest@cba7306a-a4a0-4afd-bcb4-bd19f8a24309>
Date: Fri, 30 Nov 2007 13:41:25 +0000
Subject: final version, initial import

git-svn-id: svn+ssh://mecka.net/home/svn/rtcorba-thesis@1 cba7306a-a4a0-4afd-bcb4-bd19f8a24309
---
 praes/integration.tex | 39 +++++++++++++++++++++++++++++++++++++++
 1 file changed, 39 insertions(+)
 create mode 100755 praes/integration.tex

(limited to 'praes/integration.tex')

diff --git a/praes/integration.tex b/praes/integration.tex
new file mode 100755
index 0000000..e760e70
--- /dev/null
+++ b/praes/integration.tex
@@ -0,0 +1,39 @@
+\section{Integration}
+
+\begin{frame}
+        \frametitle{RTCORBA Laserschnittstelle}
+        \begin{block}{Implementation}
+          \begin{itemize}
+		\item Schnittstelle / Komponente (Lichtweg, Laser, \dots)
+		\item Funktionen zur Parametrisierung
+		\item Funktionen zum Abruf der Statis
+	  \end{itemize}
+	\end{block}
+	\pause
+	\begin{block}{Vorteile}
+	  \begin{itemize}
+		\item Laser steuerbar via RT Ethernet
+		\item offen f\"ur zuk\"unftige Protokolle
+	  \end{itemize}
+	\end{block}
+\end{frame}
+
+\begin{frame}
+        \frametitle{DAIS}
+        \begin{block}{Data Acquisition From Industrial Systems}
+                OMG Spezifikation zur \"Uberwachung von Steuerungen:
+		\begin{itemize}
+		  \item Server, stellt Messwerte einer Steuerung zur Verf\"ugung
+		  \item Acquisitor, fordert Messwerte an (Intervall)
+		  \item Alarms \& Events, Messwerte anfordern (Grenzwerte)
+		\end{itemize}
+        \end{block}
+\end{frame}
+
+\begin{frame}
+	\frametitle{Homag DAIS}
+                \begin{center}
+		   \includegraphics[height=6cm]{../img/homagdais.jpg}
+		\end{center}
+\end{frame}
+
-- 
cgit v1.2.3

