From 824d81a0779ff3868d195ef4639d3e3eddcb69de Mon Sep 17 00:00:00 2001
From: John Ogness <john.ogness@linutronix.de>
Date: Mon, 23 Oct 2017 12:42:21 +0200
Subject: elbe: remove pauses

---
 .../elbe-overview/pres_elbe-overview_en.tex        | 32 ----------------------
 1 file changed, 32 deletions(-)

(limited to 'distribution/elbe-overview/pres_elbe-overview_en.tex')

diff --git a/distribution/elbe-overview/pres_elbe-overview_en.tex b/distribution/elbe-overview/pres_elbe-overview_en.tex
index 3afa5a0..6d935e2 100644
--- a/distribution/elbe-overview/pres_elbe-overview_en.tex
+++ b/distribution/elbe-overview/pres_elbe-overview_en.tex
@@ -12,7 +12,6 @@
 \frametitle{overview}
 \begin{block}{1) What is \includegraphics[height=0.8em]{images/elbe-logo.png}?}
 \end{block}
-\pause
 \begin{block}{2) SDCARD Image for Beaglebone Black:}
 \begin{itemize}
 \item bootloader
@@ -20,7 +19,6 @@
 \item Debian RFS (wheezy/armhf)
 \end{itemize}
 \end{block}
-\pause
 \begin{block}{3) Internals}
 \begin{itemize}
 \item resources
@@ -28,7 +26,6 @@
 \item SOAP interface
 \end{itemize}
 \end{block}
-\pause
 \begin{block}{4) Roadmap}
 \end{block}
 \end{frame}
@@ -55,7 +52,6 @@ buildroot
       \end{tabular}
     \end{column}
   \end{columns}
-\pause
 \includegraphics[width=2.5cm]{images/elbe-logo.png}
 \hspace{2em}uses Debian packages and infrastructure
 \end{frame}
@@ -65,13 +61,9 @@ buildroot
 \begin{block}{highlights}
 \begin{itemize}
 \item no more cross compiling
-\pause
 \item security
-\pause
 \item reproducible target images
-\pause
 \item cdrom with source code
-\pause
 \item licence information
 \end{itemize}
 \end{block}
@@ -89,7 +81,6 @@ create a new \includegraphics[height=0.7em]{images/elbe-logo.png} \ virtual-mach
 \begin{verbatim}
 $ elbe initvm create --build-bin --build-source example.xml
 \end{verbatim}
-\pause
 \begin{itemize}
 \item creates an elbe initvm and builds the target image and cdroms
 \end{itemize}
@@ -106,7 +97,6 @@ $ elbe initvm create --build-bin --build-source example.xml
     <primary_path>/debian</primary_path>
     <primary_proto>http</primary_proto>
 \end{lstlisting}
-\pause
 \begin{lstlisting}
     <!-- elbe-buildenv -->
     <url-list> <url> <binary>
@@ -139,7 +129,6 @@ $ elbe initvm create --build-bin --build-source example.xml
     <primary_path>/debian</primary_path>
     <primary_proto>http</primary_proto>
 \end{lstlisting}
-\pause
 \begin{lstlisting}
     <!-- kernel -->
     <url-list><url><binary>
@@ -162,14 +151,12 @@ $ elbe initvm create --build-bin --build-source example.xml
   <passwd>foo</passwd>
   <console>ttyS0,115200</console>
 \end{lstlisting}
-\pause
 \begin{lstlisting}
   <images>
     <msdoshd>
       <name>sdcard.images</name>
       <size>1900MiB</size>
 \end{lstlisting}
-\pause
 \begin{lstlisting}
         <partition>
           <size>100MB</size>
@@ -177,7 +164,6 @@ $ elbe initvm create --build-bin --build-source example.xml
           <bootable />
         </partition>
 \end{lstlisting}
-\pause
 \begin{lstlisting}
         <partition>
           <size>remain</size>
@@ -202,7 +188,6 @@ $ elbe initvm create --build-bin --build-source example.xml
       </fs>
     </bylabel>
 \end{lstlisting}
-\pause
 \begin{lstlisting}
     <bylabel>
       <label>rfs</label>
@@ -228,7 +213,6 @@ $ elbe initvm create --build-bin --build-source example.xml
     </mv>
   </finetuning>
 \end{lstlisting}
-\pause
 \begin{lstlisting}
   <pkg-list>
     <pkg>linux-image-3.12.4-rt6</pkg>
@@ -236,7 +220,6 @@ $ elbe initvm create --build-bin --build-source example.xml
   </pkg-list>
 </target>
 \end{lstlisting}
-\pause
 \begin{lstlisting}
 <!-- /boot/[MLO, uboot.images] -->
 <archive>
@@ -273,7 +256,6 @@ validation.txt
 
 are used to strip target-images
 
-\pause
 \begin{description}
 \item[setsel]
 \begin{itemize}
@@ -284,14 +266,12 @@ are used to strip target-images
 \item dpkg and perl needs to be on the target
 \end{itemize}
 
-\pause
 \item[diet]
 \begin{itemize}
 \item reverse dependency resolution
 \item postinst-scripts are executed (but may fail)
 \end{itemize}
 
-\pause
 \item[tighten]
 \begin{itemize}
 \item no dependency resolution
@@ -316,21 +296,14 @@ are used to strip target-images
 \frametitle{Packaging}
 \begin{description}
 \item[elbe-doc] man-pages, overview, XSD documentation
-\pause
 \item[elbe-common] shared python modules, XML schema
-\pause
 \item[elbe] needed on host PC (init, chg\_archive, \dots)
-\pause
 \item[elbe-buildenv] for virtual machine (buildchroot, db, chroot, \dots)
-\pause
 \item[elbe-updated] for embedded target to apply update packages
-\pause
 \item[elbe-daemon] for virtual machine (wsgi server)
-\pause
 \item[elbe-soap] for virtual machine
 	
 	implements SOAP interface
-\pause
 \item[elbe-control] for host PC
 	
 	controls SOAP interface
@@ -343,15 +316,10 @@ are used to strip target-images
 \begin{block}{technologies}
 \begin{itemize}
 	\item python
-\pause
 	\item qemu-user
-\pause
 	\item python-apt
-\pause
 	\item python-mako
-\pause
 	\item python-parted
-\pause
 	\item sqlalchemy
 \end{itemize}
 \end{block}
-- 
cgit v1.2.3

