From 6e7e1b7172813fc4ecb60597f903dd21a4616159 Mon Sep 17 00:00:00 2001
From: John Ogness <john.ogness@linutronix.de>
Date: Tue, 19 Dec 2017 11:16:28 +0100
Subject: update yocto-advanced: sync to devel/manut/yocto

The devel/manut/yocto heavily diverted from master. Sync
with latest version 8cd4956a9b48a316eab6dc6d1b1f6cd51362fecf.

Signed-off-by: John Ogness <john.ogness@linutronix.de>
---
 .../yocto-advanced/pres_yocto-advanced.tex         | 53 ++++++++++++++++------
 1 file changed, 40 insertions(+), 13 deletions(-)

(limited to 'distribution/yocto-advanced/pres_yocto-advanced.tex')

diff --git a/distribution/yocto-advanced/pres_yocto-advanced.tex b/distribution/yocto-advanced/pres_yocto-advanced.tex
index 8aabc24..13b673e 100644
--- a/distribution/yocto-advanced/pres_yocto-advanced.tex
+++ b/distribution/yocto-advanced/pres_yocto-advanced.tex
@@ -1,6 +1,7 @@
 \input{configpres}
 
 \title{YOCTO - Advanced}
+\date{}
 \maketitle
 
 \begin{frame}
@@ -9,28 +10,54 @@
 		\item Using BSP layers
 		\item Create layers \& recipes for own applications
 		\item Define a distribution
-		\item Create a customized image class
-		\item Build images
+		\item Integrate own Kernel
 \end{itemize}
 \end{frame}
 
+\input{yocto-local-conf}
 \input{yocto-layers}
-\input{yocto-ti-layer}
+%\input{yocto-wega-layer}
+\input{yocto-create-own-layer}
+\input{yocto-add-simple-application}
+\input{yocto-add-autotools-based-src}
 \input{yocto-layer-imx6}
-\input{yocto-flash-official-bb-img}
-\input{yocto-bbb-machine-conf}
 \input{yocto-add-own-kernel}
-\input{yocto-u-boot-integration}
-\input{yocto-sdcard-generation}
+%\input{yocto-flash-official-bb-img}
+%\input{yocto-bbb-machine-conf}
+%\input{yocto-u-boot-integration}
+%\input{yocto-sdcard-generation}
 \input{yocto-distro-definitions}
-\input{yocto-create-own-layer}
 \input{yocto-extend-image}
-\input{yocto-local-conf}
-\input{yocto-excercise-build-bbb-img}
-\input{yocto-add-simple-application}
-\input{yocto-add-autotools-based-src}
-\input{yocto-add-qt-cmake-projects}
+%\input{yocto-add-qt-cmake-projects}
 \input{yocto-img-customization}
+\begin{frame}[fragile]
+\frametitle{override default config files}
+default templates can be overridden by setting TEMPLATECONF
+to e.g. meta-foo/conf during ./oe-init-buildenv.
+
+Then meta-foo/conf bblayers.conf.sample and local.conf.sample will
+be used.
+
+The default location is specified in
+
+\begin{verbatim}
+% cat .templateconf
+# Template settings
+TEMPLATECONF=${TEMPLATECONF:-meta-yocto/conf}
+\end{verbatim}
+\end{frame}
+\input{yocto-scripts}
 \input{yocto-resume}
 
+\begin{frame}
+	\frametitle{Application Development Excercise}
+\begin{itemize}
+\item generate a standalone or integrated SDK
+\item configure the SDK in eclipse
+\item build and remote debug yesterdays application on the beaglebone-black
+\item integrate the application into the image
+\item build the image including your application
+\end{itemize}
+\end{frame}
+
 \input{tailpres}
-- 
cgit v1.2.3

