From 06c2add174d782eaf0841fd94678a23b20c9a383 Mon Sep 17 00:00:00 2001
From: John Ogness <john.ogness@linutronix.de>
Date: Tue, 15 May 2018 11:50:16 +0206
Subject: yocto-basic: update toolchain commands

The paths for the toolchains were too long and inconsistent with
rocko. Change them to more generic examples (using dots).

Signed-off-by: John Ogness <john.ogness@linutronix.de>
---
 distribution/yocto-basic/yocto-adt.tex | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

(limited to 'distribution/yocto-basic/yocto-adt.tex')

diff --git a/distribution/yocto-basic/yocto-adt.tex b/distribution/yocto-basic/yocto-adt.tex
index 6258653..f708b2e 100644
--- a/distribution/yocto-basic/yocto-adt.tex
+++ b/distribution/yocto-basic/yocto-adt.tex
@@ -41,20 +41,20 @@ Profiling Tools
 \begin{frame}[fragile]
 \frametitle{Build an External Usable Toolchain}
 \begin{verbatim}
-bitbake meta-toolchain
+$ bitbake meta-toolchain
 \end{verbatim}
 or to include headers and static version of all used libraries
 \begin{verbatim}
-bitbake -c populate_sdk core-image-minimal
+$ bitbake -c populate_sdk core-image-minimal
 \end{verbatim}
 To install the toolchain:
 \begin{verbatim}
-% ./tmp/deploy/sdk/poky-glibc-x86\_64-meta-toolchain-i586-toolchain-2.0.sh
-Enter target directory for SDK (default: /opt/poky/2.0): /home/devel/sdk
+$ ./tmp/deploy/sdk/poky-...-toolchain-2.4.2.sh
+Enter target directory for SDK (default: /opt/poky/2.4.2): /home/devel/sdk
 \end{verbatim}
 to use the toolchain:
 \begin{verbatim}
-source /home/devel/sdk/environment-setup-i586-poky-linux
+$ . /home/devel/sdk/environment-setup-...
 \end{verbatim}
 \end{frame}
 
-- 
cgit v1.2.3

