From cea5039322781f6085dd47954af5584ca3f78911 Mon Sep 17 00:00:00 2001
From: Jan Altenberg <jan@linutronix.de>
Date: Fri, 22 Feb 2013 12:16:22 +0100
Subject: Fix typo in Ubi handout, reported by Anna-Maria

---
 flash-memory/ubi/handout_ubi_de.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'flash-memory/ubi/handout_ubi_de.tex')

diff --git a/flash-memory/ubi/handout_ubi_de.tex b/flash-memory/ubi/handout_ubi_de.tex
index d7d03fb..15f0f8d 100644
--- a/flash-memory/ubi/handout_ubi_de.tex
+++ b/flash-memory/ubi/handout_ubi_de.tex
@@ -5,7 +5,7 @@
 \subsubsection{Was ist UBI?}
 
 UBI kann am ehesten als Logical Volume Manager (LVM) für mtd-Devices
-bezeichnet werden. Beim Start scanned UBI das mtd-Device und baut eine
+bezeichnet werden. Beim Start scant UBI das mtd-Device und baut eine
 Liste der vorhandenen Eraseblöcke auf. Dabei werden auch Bad Blocks
 richtig behandelt, da das MTD-Subsystem, auf dem UBI aufsetzt, diese
 bereits erkennt.
-- 
cgit v1.2.3

