From 692977103ba142d71c3087f953ae7b89dd283a36 Mon Sep 17 00:00:00 2001
From: John Ogness <john.ogness@linutronix.de>
Date: Thu, 31 Jan 2019 16:12:55 +0106
Subject: filesystems: change recommendations for sd-cards

ext2 is recommended for flash-based block devices? Why?!

I have changed it to F2FS and EXT4.

Signed-off-by: John Ogness <john.ogness@linutronix.de>
---
 linux-basics/filesystems/pres_filesystems_en.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'linux-basics/filesystems/pres_filesystems_en.tex')

diff --git a/linux-basics/filesystems/pres_filesystems_en.tex b/linux-basics/filesystems/pres_filesystems_en.tex
index d2c3b9e..84e4212 100644
--- a/linux-basics/filesystems/pres_filesystems_en.tex
+++ b/linux-basics/filesystems/pres_filesystems_en.tex
@@ -152,7 +152,7 @@ might be an alternative for flash devices
 \begin{frame}
 \frametitle{Recommendations}
 \begin{itemize}
-\item ''Flash-based block devices'': EXT2
+\item ''Flash-based block devices'': F2FS (EXT4 if good hardware)
 \item Block devices: EXT3, EXT4
 \item Block devices which are used in server machines (on which huge amounts
 of data are stored): XFS
-- 
cgit v1.2.3

