From 0351969fdffa9959921d8ec38b7d0d7cf095fcd0 Mon Sep 17 00:00:00 2001
From: John Ogness <john.ogness@linutronix.de>
Date: Tue, 20 Feb 2018 15:33:14 +0100
Subject: remove german slides when english are available

Remove german slides if a completely translated english version is
available. For slides that have been translated to english, but do
not contain all the information of the german slides, the german
slides are still available. But they are only available for
reference. That will not be built.

Signed-off-by: John Ogness <john.ogness@linutronix.de>
---
 realtime/rt-basics/pres_rt-basics_de.tex | 205 -------------------------------
 1 file changed, 205 deletions(-)
 delete mode 100644 realtime/rt-basics/pres_rt-basics_de.tex

(limited to 'realtime/rt-basics/pres_rt-basics_de.tex')

diff --git a/realtime/rt-basics/pres_rt-basics_de.tex b/realtime/rt-basics/pres_rt-basics_de.tex
deleted file mode 100644
index 66a78eb..0000000
--- a/realtime/rt-basics/pres_rt-basics_de.tex
+++ /dev/null
@@ -1,205 +0,0 @@
-\input{configpres}
-
-\title{Block \lq Realtime Linux\rq}
-\maketitle
-
-\subtitle{Echtzeit}
-
-\begin{frame}
-\frametitle{Was ist Echtzeit?}
-\begin{itemize}
-\item Korrektheit bedeutet auch Ausführung zum korrekten Zeitpunkt
-\item Nicht Einhalten des korrekten Zeitrahmens führt zu einem Fehler
-\end{itemize}
-\end{frame}
-
-\begin{frame}
-\frametitle{Echtzeit ''anschaulich''}
-\begin{overprint}
-\onslide<1>
-\begin{alertblock}{Wir erinnern uns}
-Nicht Einhalten des korrekten Zeitrahmens führt zu einem Fehler!
-\end{alertblock}
-\onslide<2>
-\begin{figure}[h]
-\centering
-\includegraphics[height=0.5\textwidth]{images/nuclear.png}
-\end{figure}
-\end{overprint} 
-\end{frame}
-
-\begin{frame}
-\frametitle{Anwendungsbereiche}
-\begin{itemize}
-\item Steuerungs- / Automatisierungstechnik
-\item Multimediasysteme
-\item Luft- und Raumfahrttechnik
-\item Finanzdienstleistung
-\item ...
-\end{itemize}
-\end{frame}
-
-\begin{frame}
-\frametitle{Anforderungen}
-\begin{itemize}
-\item Deterministisches Zeitverhalten
-\item Unterbrechbarkeit
-\item Priority Inheritance / Priority Ceiling
-\end{itemize}
-\end{frame}
-
-\subsubsection{Priority Inversion}
-\begin{frame}
-\frametitle{Priority Inversion}
-\begin{figure}[h]
-\centering
-\includegraphics[width=0.8\textwidth]{images/prio_inv.png}
-\end{figure}
-\end{frame}
-
-\subsubsection{Linux und Echtzeit}
-\begin{frame}
-\frametitle{Linux und Echtzeit}
-\begin{figure}[h]
-\centering
-\includegraphics[height=0.5\textwidth]{images/gpos_vs_rt.png}
-\end{figure}
-\end{frame}
-
-\begin{frame}
-\frametitle{Ansätze}
-\begin{itemize}
-\item Dual-Kernel
-\item In-Kernel / Single Kernel
-\end{itemize}
-\end{frame}
-
-\begin{frame}
-\frametitle{Dual-Kernel}
-\begin{figure}[h]
-\centering
-\includegraphics[height=0.5\textwidth]{images/dual_kernel.png}
-\end{figure}
-\end{frame}
-
-\begin{frame}
-\frametitle{Single-Kernel}
-\begin{figure}[h]
-\centering
-\includegraphics[height=0.5\textwidth]{images/single_kernel.png}
-\end{figure}
-\end{frame}
-
-\begin{frame}
-\frametitle{RTAI}
-\begin{itemize}
-\item Prof. Paolo Mantegazza, Universität Mailand
-\item Dual-Kernel Ansatz
-\item Echtzeit im Kernelspace
-\item Userspace Echtzeittasks nur eingeschränkt möglich
-\item Oberstes Designziel: Möglichst niedrige Latenzzeiten
-\item Unterstützte Plattformen: x86, x86\_64, einige ARM Plattformen
-\end{itemize}
-\end{frame}
-
-\begin{frame}
-\frametitle{RTAI}
-\begin{figure}[h]
-\centering
-\includegraphics[height=0.5\textwidth]{images/rtai.png}
-\end{figure}
-\end{frame}
-
-\begin{frame}
-\frametitle{Xenomai}
-\begin{itemize}
-\item Gegründet 2001
-\item Echtzeit im Userpace
-\item Skins bilden API verschiedenster RTOSse nach
-\item Dual-Kernel Ansatz
-\item Unterstützte Plattformen: x86, x86\_64, PowerPC, ARM, ia64
-\end{itemize}
-\end{frame}
-
-\begin{frame}
-\frametitle{Xenomai}
-\begin{figure}[h]
-\centering
-\includegraphics[height=0.5\textwidth]{images/xenomai.png}
-\end{figure}
-\end{frame}
-
-\begin{frame}
-\frametitle{Xenomai / IPIPE}
-\begin{figure}[h]
-\centering
-\includegraphics[height=0.5\textwidth]{images/ipipe.png}
-\end{figure}
-\end{frame}
-
-\begin{frame}
-\frametitle{Drum prüfe, wer sich ewig bindet...}
-\begin{overprint}
-\onslide<1>
-\begin{figure}[h]
-\centering
-\includegraphics[width=0.8\textwidth]{images/mar01.png}
-\end{figure}
-\onslide<2>
-\begin{figure}[h]
-\centering
-\includegraphics[height=0.5\textwidth]{images/mar02.png}
-\end{figure}
-\onslide<3>
-\begin{figure}[h]
-\centering
-\includegraphics[height=0.5\textwidth]{images/mar03.png}
-\end{figure}
-\end{overprint}
-\end{frame}
-
-\begin{frame}
-\frametitle{Preempt RT}
-\begin{itemize}
-\item Thomas Gleixner, Ingo Molnar
-\item In-Kernel Ansatz
-\item Große Entwicklergemeinde
-\item Viele Funktionen bereits nach ''Mainline'' Linux übernommen
-\item POSIX Realtime
-\item Hohe Akzeptanz, vollständige Integration in Linux 2006 beschlossen
-\end{itemize}
-\end{frame}
-
-\begin{frame}
-\frametitle{Preempt RT und Mainline}
-\textit{''Controlling a laser with Linux is crazy, but everyone in this room is
-crazy in his own way. So if you want to use Linux to control an industrial
-welding laser, I have no problem with your using Preempt RT''} - Linus Torvalds
-auf dem Kernel Summit 2006
-\end{frame}
-
-\begin{frame}
-\frametitle{Wie macht Preempt RT Linux echtzeitfähig?}
-\begin{overprint}
-\onslide<1>
-\begin{alertblock}{Wir erinnern uns...}
-Unterbrechbarkeit ist eine zentrale Anforderung an ein Echtzeitsystem
-\end{alertblock}
-\onslide<2>
-\begin{itemize}
-\item Locking Primitiven: Spinlocks werden durch RT Mutexe ersetzt, die schlafen
-können. Raw Spinlocks ersetzen die ursprüngliche Spinlock
-\item Interrupt Handler laufen per default in einem Kernelthread
-\end{itemize}
-\end{overprint}
-\end{frame}
-
-\begin{frame}
-\frametitle{Preempt RT}
-\begin{figure}[h]
-\centering
-\includegraphics[height=0.5\textwidth]{images/preempt_rt.png}
-\end{figure}
-\end{frame}
-
-\input{tailpres}
-- 
cgit v1.2.3

